# shared-shaping-constituent

#### Syntax

shared-shaping-constituent [ priority [ priorityValue ] | weight [ weightValue ] ]

no shared-shaping-constituent

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the attributes of implicit and explicit shared-shaping constituents and specifies explicit shared-shaping constituents. Constituents default to priority with a priority value of 8. Priority constituents are ordered before weighted constituents. The no version deletes the attributes or explicit constituent.

#### Options

- priorityValue—Value, in the range 1–8, that specifies the order in which the constituent can claim bandwidth from among all priority constituents; a lower value correlates to a higher claim; 8 is the default value
- weightValue—Value, in the range 1–31, that specifies the order in which the constituent can claim bandwidth from among all weighted constituents; a lower value correlates to a higher claim; 8 is the default value

#### Mode

Scheduler Profile Configuration

#### Related Topics

- Configuring Implicit Constituents for Simple or Compound Shared Shaping
- Configuring Explicit Constituents for Simple or Compound Shared Shaping