Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# ipv6-prefix-pool-name

#### Syntax

ipv6-prefix-pool-name poolName

no ipv6-prefix-pool-name

#### Release Information

Command introduced in JunosE Release 10.1.0.

#### Description

Specifies the IPv6 local prefix pool name to be used to delegate prefixes to the requesting router, when the RADIUS server does not return a pool name using the Framed-IPv6-Pool attribute. The no version removes the IPv6 local pool from the AAA domain map.

#### Options

- poolName—Name of the IPv6 local prefix pool to associate with the domain name; string of up to 16 alphanumeric characters

#### Mode

Domain Map Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out