Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- show dhcp-external

# Monitoring DHCP External Server Duplicate MAC Address Setting

#### Purpose

Display global configuration information for the DHCP external server application. Currently, this command displays the status of the method that DHCP external server uses to uniquely identify DHCP clients with duplicate MAC addresses.

#### Action

To display the duplicate MAC address setting for DHCP external server:

    host1#show dhcp-external
    Duplicate MAC Address: Enabled

#### Meaning

Table 1 lists the show dhcp-external command output fields.

Table 1: show dhcp-external Output Fields

Field Name | Field Description
--- | ---
Duplicate MAC Address | Status of the identification method for DHCP clients with duplicate MAC addresses: Enabled—DHCP external server uses a combination of the MAC address and giaddr to uniquely identify DHCP clients. Disabled—(Default) DHCP external server uses only the MAC address to uniquely identify DHCP clients.

#### Related Topics

- show dhcp-external

#### Published: 2010-07-20

Help
|
My Account
|
Log Out