Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- OAM Link Monitoring Feature
- Configuring 802.3ah OAM Link-Fault Management
- Example: Configuring 802.3ah OAM Link-Fault Management and Enabling Remote Failure Monitoring on an Interface

# ethernet oam lfm high-threshold

#### Syntax

[ no ] ethernet oam lfm high-threshold { disable-interface | failover }

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Configures a specific action to occur when a high threshold for an error is exceeded on an Ethernet OAM interface. The no version removes the high-threshold action from the interface of the local OAM client and causes no action to be performed when local errors occur on the interface.

#### Options

- disable-interface—Sets the OAM functionality to unconditionally attempt to influence the operational state of the interface to down. If the interface is a member link of a LAG bundle and at least one other viable link (redundant member or another active/up link) is present, OAM attempts to influence the operational state of the link to down. Otherwise, no action is taken
- failover—On GE-2 and GE-HDE line modules with GE-2 SFP I/O modules with physical link redundancy, causes the link to transition from active to redundant

#### Mode

Interface Configuration

#### Related Topics

- OAM Link Monitoring Feature
- Configuring 802.3ah OAM Link-Fault Management
- Example: Configuring 802.3ah OAM Link-Fault Management and Enabling Remote Failure Monitoring on an Interface

#### Published: 2010-07-19

Help
|
My Account
|
Log Out