Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# snmp-server group

#### Syntax

snmp-server group groupName securityModel authenticationLevel [ read readView ]
[ write writeView ] [ notify notifyView ] [ storageType ]

no snmp-server group groupName securityModel authenticationLevel

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Dynamically configures an SNMP server group. The no version removes the dynamically created group.

| Note: You must access the CLI at privilege level 15 to view or use this command.

#### Options

- groupName—Name of the SNMPv3 group
- securityModel—Security model
  - v1—SNMPv1
  - v2c—SNMPv2c
  - usm—SNMPv3
- authenticationLevel—Method for authentication and privacy
  - none—No authentication and no privacy
  - auth—Authentication only
  - priv—Authentication and privacy
- readView—Name of the view for read access; the default is no access
- writeView—Name of the view for write access; the default is no access
- notifyView—Name of the view for notification; the default is no access
- storageType—Storage type
  - volatile—Loses contents on warm or cold start
  - nonvolatile—Preserves contents across warm or cold start. This is the default.

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out