# time-to-live

#### Syntax

time-to-live ttlValue

no time-to-live

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies a hop count by setting the value of the time-to-live field used by packets sent to a RIP remote neighbor. The no version restores the default value.

#### Options

- ttlValue—Number in the range 1–16; default value is 16

#### Mode

Remote Neighbor Configuration