# Configuring Interface Sets for Scheduling and Queuing

There are a variety of tasks that you need to complete to configure a set of logical interfaces for scheduling and queuing.

To configure a set of logical interfaces:

1. Configure an interface superset.

   See Configuring Interface Supersets for QoS.

2. Configure an interface set as members of the superset.

   See Configuring Interface Sets for QoS.

3. Add interfaces as members of the interface set.

   See Adding Member Interfaces to an Interface Set.

4. Configure the scheduler hierarchy on the interface superset or the interface set.

   You can configure the scheduler hierarchy using one of the following methods:

   - Attach a QoS profile to an interface superset or an interface set. QoS profiles reference queue, drop, statistics, and scheduler profiles.

     See Attaching a QoS Profile to an Interface Superset or an Interface Set.

   - Create a QoS parameter instance on an interface superset or an interface set. QoS parameter instances enable you to configure shaping rates independent of the QoS profile and scheduler profile.

     See Creating a QoS Parameter on an Interface Superset or Interface Set.

5. (Optional) Monitor the configuration of interface sets and supersets.

   See Monitoring the Configuration of QoS Interface Sets and Monitoring the Configuration of QoS Interface Supersets.

#### Related Documentation

- Interface Sets for QoS Overview