# baseline radius dynamic-request

#### Syntax

baseline radius dynamic-request

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for RADIUS dynamic-request statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Mode

Privileged Exec

#### Related Documentation

- Monitoring Packet Mirroring Overview