Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show isis database

#### Syntax

show isis database [ level-1 | level-2 | l1 | l2 | lspid | hostname | detail | verbose ]*
[ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
hostname variable added in JunosE Release 7.3.0.

#### Description

Displays the IS-IS link-state database.

#### Options

- level-1—Displays the IS-IS link-state database for level 1
- level-2—Displays the IS-IS link-state database for level 2
- l1—Displays the IS-IS link-state database for level 1
- l2—Displays the IS-IS link-state database for level 2
- lspid—Link-state PDU identifier in the form xxxx.xxxx.xxxx.yy.zz; when specified, displays the contents of a single link-state PDU by its ID number
- hostname—Displays the IS-IS link-state database for the specified hostname
- detail—Additionally displays contents of each link-state PDU; if not specified, a summary display is provided
- verbose—Additionally displays MPLS traffic engineering information
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out