# ipv6 http redirectUrl

#### Syntax

ipv6 http redirectUrl url

no ipv6 http redirectUrl

#### Release Information

Command introduced in JunosE Release 10.1.0.

Profile Configuration mode added in JunosE Release 11.0.0.

#### Description

Specifies the URL to which a subscriber's initial Web browser session is redirected, enabling initial provisioning and service selection for the subscriber. The no version removes the redirection action.

#### Options

- url—Name of the URL; 64 characters maximum

#### Mode

Interface Configuration, Subinterface Configuration, Profile Configuration

#### Related Documentation

- Configuring the HTTP Server to Support Guided Entrance in the JunosE Broadband Access Configuration Guide