# dhcpLocalProtocol

#### Description

DHCP local server protocol

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Cannot find interface; remote client bind add failed; client failed to decline IP address; client failed to decline a null offered IP address; delete remote client entry failed

#### Warning Log

AAA not responding; SDX program not responding; rediscovering with no IP address allocated; a renewal is received on the line module for an unknown client; secondary DNS without primary DNS configured, using DHCP values; secondary NetBIOS Name Server (NBNS) without primary NBNS configured, using DHCP values; duplicate MAC address detected

#### Notice Log

None

#### Info

None

#### Debug

Received packet; transmit packet; authentication status; DHCP local server state transitions

#### Filter

interface interfaceType interfaceSpecifier

- interface—Logs events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.