# ip flow-aggregation cache

#### Syntax

[ no ] ip flow-aggregation cache [ as | destination-prefix | prefix | protocol-port | source-prefix ]

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Creates an aggregation cache and accesses Flow Cache Configuration mode. The no version removes the aggregation cache and its configuration.

#### Options

- as—Specifies autonomous system aggregation
- destination prefix—Specifies destination prefix aggregation
- prefix—Specifies prefix aggregation
- protocol-port—Specifies protocol port aggregation
- source-prefix—Specifies source prefix aggregation

#### Mode

Flow Cache Configuration, Global Configuration