# discovery-mode

#### Syntax

[ no ] discovery-mode

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Enables ANCP discovery mode. This mode allows RADIUS software to obtain loop parameter information from a connected access node. If discovery mode is disabled, it does not accept topology discovery messages and stops advertising topology discovery capability. It does not affect any other neighbors. The no version disables ANCP discovery mode.

#### Mode

L2C Neighbor Configuration