# aaaServerGeneral

#### Description

AAA server general

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Subscriber count exceeds license plus grace; internal attachment errors

#### Warning Log

Subscriber count exceeds license; cannot grow internal memory pools; accounting message failures; the Framed-IPv6-Prefix RADIUS attribute is used for both IPv6 Neighbor Discovery router advertisements and DHCPv6 Prefix Delegation;Notify duplicate event ignored for profileHandle: profileHandle issu in progress; Notify duplicate event ignored for profileHandle: profileHandle unable to allocate memory

#### Notice Log

Authentication failures resulting from memory allocation failures

#### Info

None

#### Debug

Authentication failures resulting from reasons other than memory allocation failures; status of authentication; accounting and address assignment requests sent to local (internal) servers; duplicate accounting message failures; EAP challenge received; memory allocation failure for tunnel definition table and profile; failed to insert tunnel attribute and tunnel tag table; container size exceeded: creating new; found unexpected tunnel table; dsl-forum atrribute type parse error: limited data or overflow; Duplicate prefix event received for profileHandle: profileHandle

#### Filter

None