Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# snmp-server community

#### Syntax

snmp-server community commString [ view viewName ] [ priv ] [ accessListName ]

no snmp-server community commString

#### Release Information

Command introduced before JunosE Release 7.1.0.
view keyword and viewName variable added in JunosE Release 7.1.0.

#### Description

Configures an authorized SNMP community and associates SNMPv1/v2c communities with SNMPv3 views. The no version removes an authorized community from the list of communities.

#### Options

- commString—Name of the SNMPv1/v2c community
- viewName—Name of the SNMPv3 view, which allows configuration using available dynamic views
- priv—Privileged Exec level: ro (read-only), rw (read-write), or admin (administrator)
- accessListName—Name of IP access list to filter SNMP clients

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out