# ip share-interface

#### Syntax

ip share-interface interfaceType interfaceSpecifier

no ip share-interface

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the layer 2 interface that an IP interface will share in the current virtual router. The no version removes the association between the layer 2 interface and the shared IP interface.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Interface Configuration