# Monitoring Active IP Subscribers Created by Subscriber Management

#### Purpose

Display information about active IP subscribers that were created by the JunosE Software’s subscriber management feature.

#### Action

To display information about subscribers that were created by subscriber management:

    host1# show ip-subscriber 2835349506
                                                Virtual
        Id         User Name      Ip Address    Router      Interface
    ----------   --------------   -----------   -------   -------------
    2835349506   user1@isp1.com   192.168.0.1   default   ip192.168.0.1
        Id         Login time
    ----------   ------------------------
    2835349506   WED AUG 23 20:46:24 2006

    host1# show ip-subscriber detail
                                 Subscriber List
                                 ---------------
                                                Virtual
        Id         User Name      Ip Address    Router      Interface
    ----------   --------------   -----------   -------   -------------
    2835349506   user1@isp1.com   192.168.0.1   default   ip192.168.0.1
                                                             Profile
        Id              Login Time           Mac Address      Handle
    ----------   ------------------------   --------------   --------
    2835349506   WED AUG 23 20:46:24 2006   3000.0001.9365   13631489
                 Interface   Service
        Id        Profile    Profile        Option 82
    ----------   ---------   ---------   ----------------
    2835349506   myProfile   profile22   FastEthernet 3/1

#### Meaning

Table 137 lists the show ip-subscriber command output fields.

Table 137: show ip-subscriber Output Fields

Field Name | Field Description
--- | ---
Id | ID of the subscriber
User Name | Username used to retrieve information from RADIUS for the subscriber interface
Ip Address | IP address of the subscriber interface
Virtual Router | Name of the virtual router on which the subscriber interface is configured
Interface | Name of subscriber interface; ip indicates that subscriber manager created this interface
Login Time | Day, date, and time that the subscriber logged in
Mac Address | MAC address of the subscriber
Profile Handle | AAA profile handle
Interface Profile | Interface profile name used to configure the subscriber interface
Service Profile | IP service profile name used by subscriber management to authorize and configure the subscriber interface with AAA
Option 82 | DHCP relay agent information (option 82) circuit identifier that describes the physical interface location associated with the subscriber

#### Related Documentation

- show ip-subscriber