# show ip pim interface

#### Syntax

show ip pim interface { summary | [ interfaceType interfaceSpecifier ] [ count ]
[ filter ] }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information about each PIM dense mode interface.

#### Options

- summary—Displays the number of configured, enabled, and disabled PIM dense mode, PIM sparse mode, and PIM sparse-dense mode interfaces
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- count—Displays the number of incoming and outgoing PIM control packets
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec