# ip nat inside source static

#### Syntax

[ no ] ip nat inside source static localIpAddress globalIpAddress

[ no ] ip nat inside source static { tcp | udp } localIpAddress localPort globalIpAddress globalPort

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates static translations for a source address when routing a packet from the inside network to the outside network, and “ untranslates” the destination address when a packet returns from the outside network to the inside network. The no version removes the static translation and purges the associated translations from the translation table.

#### Options

- tcp—Indicates a TCP port
- udp—Indicates a UDP port
- localIpAddress—Inside local address
- localPort—Inside local TCP or UDP port
- globalIpAddress—Inside global address
- globalPort —Inside global TCP or UDP port

#### Mode

Global Configuration