# ripRoute

#### Description

RIP route

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

None

#### Debug

Routes sent or received by RIP; if a route is rejected or not sent, gives the reason

#### Filter 1

interface interfaceType interfaceSpecifier

- interface—Logs PPP events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.

#### Filter 2

router virtualRouterName

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events