# clear ip tunnel-routes

#### Syntax

clear ip tunnel-routes [ vrf vrfName ] { * | ipAddress ipMask }

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Clears and then refreshes a specified route or all dynamic routes from the tunnel routing table of the virtual router or a specified VRF. There is no no version.

#### Options

- vrfName—Name of the VRF context from which routes are to be cleared
- *—Clears all dynamic routes
- ipAddress—IP address prefix for routes that are cleared; in 32-bit dotted-decimal format
- ipMask—Mask of the IP address prefix for routes that are cleared; in 32-bit dotted-decimal or /N format

#### Mode

Privileged Exec