# Monitoring AS-Path Access Lists

#### Purpose

Display AS-path access lists.

#### Action

To display AS-path access lists:

    host1#show ip as-path-access-list
    AS Path Access List 10:
      permit [200-220]
      permit ^114
      permit ^117.*225$
    AS Path Access List 11:
      deny .*
    AS Path Access List 20:
      deny [1100-1250]
      permit .*

#### Meaning

Table 24 lists the show ip as-path-access-list command output fields.

Table 24: show ip as-path-access-list Output Fields

Field Name | Field Description
--- | ---
As Path Access List | Name of an AS Path Access List
permit, deny | Condition statement for routes matching the condition

#### Related Documentation

- show ip as-path-access-list