# ip dhcp-local auth password

#### Syntax

[ no ] ip dhcp-local auth password password

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Assigns a password used to authenticate a locally configured DHCP standalone mode client. In DHCP standalone mode, the password is presented to AAA in an authentication request. The no version removes the password.

#### Options

- password—String of 1–32 characters used as the password

#### Mode

Global Configuration