# show ip interface

#### Syntax

show ip interface [ vrf vrfName ]
{ { [ brief | detail | other | show-virtual-router [ virtualRouterName ] ]
[ interfaceType interfaceSpecifier ] } | summary } [ delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
show-virtual-router keyword and virtualRouterName variable added in JunosE Release 7.3.0.
other keyword added in JunosE Release 8.0.0.

#### Description

Displays current state of all IP interfaces or the IP interfaces you specify. The default is all interface types and all interfaces.

#### Options

- vrfName—Name of the VRF
- brief—Displays a brief summary of IP status and configuration information
- detail—Shows a detailed display of IP status and configuration information
- other—Shows hidden interfaces and routes to the local address that are used internally so that from a given CE you can now ping the local address of any VRF that has a VPN overlapping a VPN to which the CE belongs
- virtualRouterName—Name of the virtual router
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- summary—Shows a detailed summary of IP status and configuration
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring the QoS Configuration of IP Interfaces
- Monitoring the Policy Configuration of IP Interfaces
- Monitoring the Packet Mirroring Configuration of IP Interfaces