# radius trap no-auth-server-responding

#### Syntax

radius trap no-auth-server-responding { enable | disable }

no radius trap no-auth-server-responding

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables or disables SNMP traps when all the configured RADIUS authentication servers per VR fail to respond to a RADIUS Access-Request message. The no version restores the default, disable.

#### Options

- enable—Specifies the feature
- disable—Disables the feature; this is the default setting

#### Mode

Global Configuration