# ntp enable

#### Syntax

[ no ] ntp enable

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables NTP services on the router and attaches the NTP client to the current virtual router. The no version disables reception of NTP packets on the router and removes the association between NTP and the virtual router. The default setting is disable.

#### Mode

Global Configuration