# Setting the MLD Proxy Baseline

You can set the counters for the numbers of queries received and reports sent on the upstream interface to zero. This feature allows you to establish a reference point for MLD proxy statistics.

baseline ipv6 mld-proxy interface

- Use to set the counters for the numbers of queries received and reports sent on the upstream interface to zero.

  | Note: Issue this command only on the upstream interface. Otherwise, this command will have no effect.

- Example
  (host1)#baseline ipv6 mld-proxy interface
- There is no no version.
- See baseline ipv6 mld-proxy interface.