# ipsec isakmp-policy-rule

#### Syntax

ipsec isakmp-policy-rule priority

no ipsec isakmp-policy-rule [ priority ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines and prioritizes an ISAKMP/IKE policy. ISAKMP/IKE policies define parameters to be used during ISAKMP/IKE negotiation. You can have up to 10 ISAKMP/IKE policies per router. The no version removes a policy. If you do not include a priority number with the no version, the software removes all ISAKMP/IKE policies.

| Note: This command has been replaced by the ipsec ike-policy-rule command and may be removed completely in a future release.

#### Options

- priority—Identifies and prioritizes the ISAKMP/IKE policy; in the range 1–10000, with 1 having the highest priority

#### Mode

Global Configuration