# include circuit-identifier

#### Syntax

include circuit-identifier circuitType [ prepend-circuit-type ]

no include circuit-identifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies that the circuit identifier is included when the router automatically generates a username for an IP service profile. The no version disables inclusion of the circuit identifier.

#### Options

- circuitType—Type of circuit; atm or vlan
- prepend-circuit-type—Specifies that the circuit type is included in the username

#### Mode

IP Service Profile Configuration