# show bridge interface vpls

#### Syntax

show bridge interface vpls vplsName [ delta ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Displays configuration, statistics, and status information for a VPLS instance on the VPLS virtual core interface, which represents all the MPLS tunnels from the router to the remote VPLS edge (VE) devices.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec

#### Related Documentation

- Monitoring Configuration, Statistics, and Status for VPLS Core Interfaces in the JunosE BGP and MPLS Configuration Guide