Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# service-management owner-session

#### Syntax

[ no ] service-management owner-session ownerName ownerId
service-session serviceName [ service-session-profile profileName ]

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Activates subscriber service sessions based on the specified owner and owner-generated ID. The no version gracefully removes the specified service session for the specified owner session.

Privileged Exec mode creates a dynamic subscriber service session that is deleted after a router reboot. Global Configuration mode creates a persistent service session.

#### Options

- ownerName—Name of the owner for the owner session; AAA for RADIUS-based subscribers
- ownerId—Unique ID that is generated by the owner; Acct-Session-ID for AAA subscriber sessions
- serviceName—Name of the service session to use
- profileName—Name of the service session profile to use for the service session

#### Mode

Global Configuration, Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out