# forwarding-rate-threshold

#### Syntax

forwarding-rate-threshold forwardingRateThreshold

no forwarding-rate-threshold

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the threshold above which forwarded-rate-exceeded events are logged. The no version removes the threshold.

#### Options

- forwardingRateThreshold—Bits per second in the range 0–1073741824

#### Mode

Statistics Profile Configuration

#### Related Documentation

- Configuring Event Statistics