# Creating Policy Lists for VLANs

The following example creates a VLAN policy list named routeForVlan. The classifier group lowLatencyLowDrop uses the default precedence of 100.

1. Create the policy list routeForVlan.
   host1(config)#vlan policy-list routeForVlan host1(config-policy-list)#
2. Create the classification group.
   host1(config-policy-list)#classifier-group lowLatencyLowDrop host1(config-policy-list-classifier-group)#
3. Create a rule that adds the lowLatencyLowDrop traffic class for all packets that fall into the lowLatencyLowDrop classification.
   host1(config-policy-list-classifier-group)#traffic-class lowLatencyLowDrop
4. Add a rule that sets the drop precedence for all packets that fall into the lowLatencyLowDrop classification to green.
   host1(config-policy-list-classifier-group)#color green
5. Add a rule that sets the user-priority bits for all packets that fall into the lowLatencyLowDrop classification to 7.
   host1(config-policy-list-classifier-group)#mark-user-priority 7
6. Exit to Policy List Configuration mode, then add traffic class rules for packets that conform to different CLACLs.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group lowLatency host1(config-policy-list-classifier-group)#traffic-class lowLatency host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group excellentEffort host1(config-policy-list-classifier-group)#traffic-class excellentEffort host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group bestEffort host1(config-policy-list-classifier-group)#traffic-class bestEffort
7. Exit Policy List Configuration mode to save the configuration.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#exit host1(config)#
8. Display the policy list.

       host1#show policy-list routeForVlan

                                         Policy Table
                                         ------ -----
       VLAN Policy routeForVlan
          Administrative state: enable
          Reference count:      0
          Classifier control list: lowLatencyLowDrop, precedence 100
             traffic-class lowLatencyLowDrop
             color green
             mark-user-priority 7
          Classifier control list: lowLatency, precedence 100
             traffic-class lowLatency
          Classifier control list: excellentEffort, precedence 100
             traffic-class excellentEffort
          Classifier control list: bestEffort, precedence 100
             traffic-class bestEffort

#### Related Documentation

- vlan policy-list