# yellow-mark

#### Syntax

[ no ] yellow-mark colorMarkValue

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Applies ToS mark value to yellow packets, which can be from policy actions, earlier policies, or rate-limit hierarchies. The no version deletes the ToS mark value.

#### Options

- colorMarkValue—Value of the ToS mark to be applied, in the range 0–255

#### Mode

Color Mark Profile Configuration

#### Related Documentation

- Hierarchical Rate Limits Overview
- Policy Rule Precedence