# bgp confederation peers

#### Syntax

bgp confederation peers { autonomousSystem [ autonomousSystem ]* |
filter-list filterListName }

no bgp confederation peers [ autonomousSystem [ autonomousSystem ]* |
filter-list filterListName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the sub-ASs that belong to a confederation by listing individual AS numbers or by reference to an AS-path access list (the filter list). If the remote AS of a peer appears in the list of sub-AS numbers or in the filter list, then the peer is considered to be in the same confederation. The no version removes individually specified sub-ASs, all sub-ASs specified by the filter list, or all sub-ASs from the confederation.

#### Options

- autonomousSystem—AS number in the range 1– 4294967295
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filterListName—Name of an AS-path access list; a string of up to 32 characters

#### Mode

Router Configuration