# ipv6 mld access-source-group

#### Syntax

ipv6 mld access-source-group accessListName

no ipv6 mld access-source-group

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Restricts hosts on this subnetwork to membership in those source groups (also known as “ channels” ) permitted by the specified IPv6 access list. The no version removes any access list restriction.

#### Options

- accessListName—Name of the access list; a string of up to 32 characters

#### Mode

Interface Configuration, Profile Configuration