# baseline clns

#### Syntax

baseline clns [ interfaceType interfaceSpecifier ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for CLNS. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec