# Monitoring LDP Targeted Hello Receive and Send Lists

#### Purpose

Display LDP targeted hello receive or send list, or both.

#### Action

To display both the LDP targeted hello receive and send lists:

    host1#show ldp targeted session
    Mpls Target Session Status:

     D = Dynamically, S = Statically, A = Access List Configured

        Targeted session sent to 10.9.1.3 is up  Used By: D
          indirect nexthop index 3, resolved
        Targeted session sent to 10.9.1.6 is up  Used By: S
          indirect nexthop index 206, resolved

#### Meaning

Table 71 lists the show ldp targeted session command output fields.

Table 71: show ldp targeted session Output Fields

Field Name | Field Description
--- | ---
D | Targeted session created by layer 2 over MPLS connection; see Layer 2 Services over MPLS Overview in the JunosE BGP and MPLS Configuration Guide for more information about layer 2 over MPLS
S | Targeted session statically created by user
A | Targeted session created by access list
Used By | Letter representing source of targeted session

#### Related Documentation

- show ldp targeted session