# isisGeneral

#### Description

IS-IS system notifications

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Error in restoring NVS

#### Warning Log

Exceeding maximum IP addresses on interface or maximum sequence number

#### Notice Log

Error in redistributing routes; LAN circuit coming up; BGP converged; BGP not converged and IS-IS times out; transient black hole avoidance suppressed because graceful restart has been configured and is in progress

#### Info

None

#### Debug

Redistributed routes

#### Filter 1

interface—See description of the isisAdjChange interface filter for information about this filter

#### Filter 2

router—See description of the isisAdjChange router filter for information about this filter