# ip dvmrp route-limit

#### Syntax

[ no ] ip dvmrp route-limit [ limit ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Limits the number of routes that the router can advertise on each interface. The default value is 7000. The no version removes the limit for the number of routes that the router can advertise on each interface.

#### Options

- limit—Number of routes that the router can advertise

#### Mode

Global Configuration