# deadtime

#### Syntax

deadtime recovery

no deadtime

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the amount of time, in minutes, that a server is marked as unavailable if a request times out for the configured retry count. If a server fails to answer a request, it is marked “ unavailable” by the router. The router does not send requests to the server for the configured time. The no version restores the default value, 0, turning off the deadtime mechanism.

#### Options

- recovery—Number of minutes that a server is marked as unavailable, in the range 0–1440; default value is 0

#### Mode

RADIUS Configuration