Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Strict-Priority and Relative Strict-Priority Scheduling Overview
- For more information about specifying an expression that you can reference within a scheduler profile, see Using Expressions for Bandwidth and Burst Values in a Scheduler Profile
- node
- qos-profile
- scheduler-profile
- shaping-rate
- weight

# Configuring Relative Strict-Priority Scheduling for Aggregate Shaping Rates

To configure relative strict priority scheduling for aggregate shaping rates:

1. Create a scheduler profile for the strict-priority queue.
   host1(config)# scheduler-profile relativeStrict host1(config-scheduler-profile)# shaping-rate 500000 host1(config-scheduler-profile)# weight 0 host1(config-scheduler-profile)# exit

   Configuring the weight of 0 reduces latency and jitter.

2. Create a scheduler profile for the nonstrict best-effort queue.
   host1(config)# scheduler-profile be host1(config-scheduler-profile)# shaping-rate 1000000 burst 1 host1(config-scheduler-profile)# weight 8 host1(config-scheduler-profile)# exit

   | Tip: If you need to impose a shaping rate on the nonstrict queues to meet a functional requirement, you can specify a rate less than the aggregate rate. The key is that the burst size must be one, or small. The burst size determines the maximum-sized packet that can squeeze in front of a relative strict-priority packet in the round robin.

3. Create a scheduler profile for the aggregate bandwidth.
   host1(config)#scheduler-profile vcAggregate host1(config-scheduler-profile)#shaping-rate 1000000 host1(config-scheduler-profile)#exit
4. Create a QoS profile, configure node shaping for each queue, and add each of the queues to the QoS profile.
   host1(config)# qos-profile relative-strict-aggregate host1(config-qos-profile)# atm-vc node scheduler-profile vcAggregate host1(config-qos-profile)# atm-vc queue traffic-class best-effort
   scheduler-profile be host1(config-qos-profile)# atm-vc queue traffic-class voice scheduler-profile relativeStrict host1(config-qos-profile)# exit host1(config)#

This configuration creates the hierarchy shown in Figure 1.

Figure 1: Sample Relative Strict-Priority Scheduler Hierarchy

## Related Documentation

- Strict-Priority and Relative Strict-Priority Scheduling Overview
- For more information about specifying an expression that you can reference within a scheduler profile, see Using Expressions for Bandwidth and Burst Values in a Scheduler Profile
- node
- qos-profile
- scheduler-profile
- shaping-rate
- weight

#### Published: 2010-12-20

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out