# tunnel mpls fast-reroute

#### Syntax

[ no ] tunnel mpls [ traffic-eng ] fast-reroute

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures local protection for the ingress router of the primary LSP by causing RSVP-TE to signal at LSP setup that the primary LSP needs local protection. The no version removes the configuration.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations

#### Mode

Interface Configuration