Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Strict-Priority and Relative Strict-Priority Scheduling Overview
- For more information about specifying an expression that you can reference within a scheduler profile, see Using Expressions for Bandwidth and Burst Values in a Scheduler Profile
- group
- node
- qos-profile
- queue
- scheduler-profile
- shaping-rate
- strict-priority
- traffic-class
- traffic-class-group

# Configuring Strict-Priority Scheduling

To configure strict-priority scheduling:

1. Configure the traffic classes.
   host1(config)#traffic-class Low-loss-1 host1(config-traffic-class)#exit host1(config)#traffic-class Low-latency-1 host1(config-traffic-class)#exit host1(config)#traffic-class Low-latency-2 host1(config-traffic-class)#exit
2. Configure the auto-strict-priority traffic-class group, and add the traffic classes that must receive strict-priority scheduling to the group.
   host1(config)#traffic-class-group Strict-priority auto-strict-priority host1(config-traffic-class-group)#traffic-class Low-latency-1 host1(config-traffic-class-group)#traffic-class Low-latency-2 host1(config-traffic-class-group)#exit
3. Create a scheduler profile for strict-priority traffic and configure the shaping rate.
   host1(config)#scheduler-profile strictPriorityBandwidth host1(config-scheduler-profile)#shaping-rate 20000000 host1(config-scheduler-profile)#exit
4. Configure a QoS profile.
   host1(config)#qos-profile Example-qos-profile host1(config-qos-profile)#atm group default host1(config-qos-profile)#atm group Strict-priority scheduler-profile strictPriorityBandwidth host1(config-qos-profile)#atm-vc node group default host1(config-qos-profile)#atm-vc node group Strict-priority host1(config-qos-profile)#atm-vc queue traffic-class best-effort host1(config-qos-profile)#atm-vc queue traffic-class Low-loss-1 host1(config-qos-profile)#atm-vc queue traffic-class Low-latency-1 host1(config-qos-profile)#atm-vc queue traffic-class Low-latency-2 host1(config-qos-profile)#exit
5. Attach the QoS profile to an interface.
   host1(config)#interface atm 2/0 host1(config-if)#qos-profile Example-qos-profile host1(config-if)#exit host1(config)#

This configuration creates the hierarchy shown in Figure 1.

Figure 1: Sample Strict-Priority Scheduling Hierarchy

## Related Documentation

- Strict-Priority and Relative Strict-Priority Scheduling Overview
- For more information about specifying an expression that you can reference within a scheduler profile, see Using Expressions for Bandwidth and Burst Values in a Scheduler Profile
- group
- node
- qos-profile
- queue
- scheduler-profile
- shaping-rate
- strict-priority
- traffic-class
- traffic-class-group

#### Published: 2010-12-20

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out