Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Using Policy Rules to Provide Routing Solutions

The next-interface, next-hop, filter, and forward rules provide routing solutions for traffic matching a classifier. A classifier can have only one action that provides a routing solution.

If you configure two routing solution rules, such as filter and forward, in the same classifier group, the router displays a warning message, and the rule configured last replaces the previous rule.

For IP policy lists, policy rules are available to enable you to make a forwarding decision that includes the next interface and next hop:

- Forward next interface—Causes an interface to forward all packets that satisfy the classification associated with that rule to the next interface specified
- Forward next hop—Causes an interface to forward all packets that satisfy the classification associated with that rule to the next-hop address specified

For example, you can route packets arriving at IP interface ATM 0/0.0 so that they area handled as indicated:

- Packets from source 1.1.1.1 are forwarded out of interface ATM 0/0.1.
- Packets from source 2.2.2.2 are forwarded out of interface ATM 2/1.1.
- All other packets are dropped.

To configure this routing policy, issue the following commands:

host1(config)#ip classifier-list claclA ip host 1.1.1.1 any host1(config)#ip classifier-list claclB ip host 2.2.2.2 any host1(config)#ip policy-list IpPolicy100 host1(config-policy-list)#classifier-group claclA host1(config-policy-list-classifier-group)#forward interface atm 0/0.1 host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group claclB host1(config-policy-list-classifier-group)#forward interface atm 2/1.1 host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group * host1(config-policy-list-classifier-group)#filter host1(config-policy-list-classifier-group)#exit host1(config)#interface atm 0/0.0 host1(config-subif)#ip policy input IpPolicy100 statistics enabled

#### Published: 2010-12-28

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out