# baseline ipv6 mld

#### Syntax

baseline ipv6 mld

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a baseline for MLD statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Mode

Privileged Exec