# mpls tunnel-model

#### Syntax

mpls tunnel-model { pipe | uniform }

no mpls tunnel-model

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies whether MPLS employs the pipe or uniform tunnel model for differentiated services. The no version restores the default, the pipe model.

#### Options

- pipe-model—Specifies that the pipe model is followed
- uniform-model—Specifies that the uniform model is followed

#### Mode

Global Configuration