# l2c oam

#### Syntax

l2c oam { neighbor neighborName end-user-id endUserId | interface interfaceType interfaceSpecifier } [ count countValue ] [ timeout timeoutValue ]

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Triggers the access node to run a local loopback test on the specified interface. There is no no version.

#### Options

- neighborName—Name of the neighbor
- endUserId—Output ANCP label
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- countValue—Number of local loopback messages
- timeoutValue—Time (in seconds) for the access node to wait for a loopback response from the neighbor

#### Mode

Privileged Exec, User Exec