# mirror analyzer-ip-address

#### Syntax

mirror analyzer-ip-address analyzerIpAddress analyzer-virtual-router vrName
[ analyzer-udp-port udpPort [ mirror-identifier mirrorId
[ session-identifier sessionId ] ] ]

no mirror

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the mirror action for a classifier group in a secure IP or L2TP policy list. The no version deletes the mirror rule.

#### Options

- analyzerIpAddress—IP address of the analyzer
- vrName—Name of the virtual router where the analyzer interface is configured
- udpPort—UDP port of the analyzer; required for L2TP packet mirror rules
- mirrorId—Mirror identifier
- sessionId—Session identifier

#### Mode

Classifier-Group Configuration

#### Related Documentation

- Configuring CLI-Based Mirroring