# mpls traffic-eng multicast-intact

#### Syntax

[ no ] mpls traffic-eng multicast-intact

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Enables a multicast network and MPLS traffic engineering (TE) network to interoperate on a router running OSPF. The no version disables interoperability between multicast protocols and MPLS-TE.

#### Mode

Router Configuration